매립장 지하수 검사정의 수질특성 조사

박혜진, 서윤규, 이재령, 정혜민, 노형석, 유지혜, 김민지, 박혜영, 안길원

수질분석과

Characteristics of Water Quality

in Landfill Groundwater Monitoring Wells

H. J. Park, Y. G. Seo, J. R. Lee, H. M. Jung, H. S. Noh, J. H. Yu,

M. J. Kim, H. Y. Park, G. W. Ahn.

Water Quality Analysis Division

Abstract

This study analyzed groundwater quality data collected from monitoring wells installed in Yeosu, Suncheon, and Gwangyang in Jeollanam-do, between 2015 and 2024. The objective of this study was to evaluate long-term trends in groundwater quality and to investigate the impact of landfill leachate. Key parameters analyzed included pH, BOD, COD, chloride(Cl⁻), nitrate nitrogen(NO3-N), ammonia nitrogen(NH3-N), and heavy metals. Over the ten-year monitoring period, most parameters met the national standards for domestic groundwater use, indicating generally stable groundwater conditions.

However, some areas exhibited noticeable changes in specific parameters. In the Yeosu Manheung and Wollae sites, little difference was observed between upstream and downstream wells, suggesting minimal impact from leachate. In contrast, the Suncheon site showed consistently high concentrations of COD and chloride. After 2019, concentrations in downstream well 1 began to decline, while those in downstream well 2 remained high, indicating potential localized contamination or changes in groundwater flow direction. In Gwangyang, groundwater conditions generally remained stable. However, a growing difference in nitrate nitrogen concentrations between upstream and downstream wells suggests the need for continued monitoring. This study provides foundational data for managing groundwater contamination in the study sites and contributes to the development of effective leachate monitoring systems.

Key words : Landfill, Groundwater monitoring well

2015년부터 2024년까지 10년간 여수, 순천, 광양 지역 매립장 지하수 검사정의 수질 특성 조사 결과는 다음과 같다.

1. 수소이온 농도는 생활용수 수질기준인 5.8 ~ 8.5 범위를 만족하는 안정적인 수준을 유지하였다. BOD는 여수 만흥, 월내, 순천, 광양 매립장 모두 평균 1.0 mg/L 미만의 낮은 농도를 보였다. COD의 경우 여수 만흥 0.2 mg/L ~ 6.7 mg/L(평균 1.8 mg/L), 여수 월내 0.1 ~ 7.8 mg/L(평균 1.8 mg/L), 순천 0.3 mg/L ~ 10.8 mg/L(평균 4.4 mg/L), 광양 ND ~ 4.8 mg/L(평균 0.8 mg/L)의 농도로 나타났다.

2. 염소이온은 여수 만흥 2.4 mg/L ~ 45.4 mg/L(평균 16.5 mg/L), 여수 월내 9.8 mg/L ~ 136.3 mg/L(평균 49.2 mg/L), 순천 8.0 mg/L ~ 313.8 mg/L(평균 122.6 mg/L), 광양 3.7 mg/L ~ 64.7 mg/L(평균 11.3 mg/L)의 농도로 나타났다.

3. 질산성질소는 여수 만흥 0.5 mg/L ~ 13.1 mg/L(평균 4.4 mg/L), 여수 월내 ND ~ 18.9 mg/L(평균 3.5 mg/L), 순천 ND ~ 4.1 mg/L(평균 1.0 mg/L), 광양 ND ~ 5.6 mg/L(평균 1.9 mg/L) 의 농도로 생활용수 기준인 20 mg/L을 초과하지 않았다. 암모니아성질소는 대부분 검출되지 않거나 0.5 mg/L 미만으로 검출되었다.

4. 중금속, 휘발성유기화합물, 시안, 페놀, 유기인계 농약 농도를 분석한 결과 대부분의 항목이 검출되지 않았다. 일부 항목이 미량 검출되거나 일시적으로 생활용수 기준을 초과하는 사례가 확인되었으나 대체로 일회성에 그쳤으며, 지속적인 증가 경향이나 광범위한 오염 양상은 관찰되지 않았다.

5. 여수 만흥, 여수 월내, 광양 매립장은 상·하부 검사정 간 농도 차이가 크지 않아 지하수 흐름이 안정적인 것으로 분석되었다. 반면 순천 매립장은 COD, 염소이온, 질산성질소 항목에서 하부 1지점에 한해 뚜렷한 농도 변화가 나타났다. 이는 지하수 유동 변화나 외부 요인의 영향을 시사하며, 침출수 영향 파악을 위한 추가 모니터링이 필요한 것으로 판단된다.