전라남도 지정 명품 지하수 발굴(Ⅴ)

이소영, 이정일, 김민영, 장성국, 임형인, 김지우, 남지현,

박귀님, 박귀환, 박종수

수질분석과

A study on the Assessment of Superior Groundwater Resources in Jeollanam-do(Ⅴ)

S. Y. Lee, J. I. Lee, M. Y. Kim, S. G. Jang, H. I. Lim, G. W. Kim,

J. H. Nam, G. N. Park, G. H. Park, J. S. Park

Water Quality Analysis Division

Abstract

This study was conducted to locate the groundwater in which the water quality is very good and the variability of water quality is low in the Jeollanam-do region. Samples were extracted from 63 sites from the soil ground water information system(SGIS), the national water works information system(NWIS), and recommended sites by the towns and provincial offices in Jeollanam-do(total 23,450 sites). The criteria for the candidates were as follows: Suitable for natural mineral water standard, the range of pH is 7.0 ~ 8.5, the amount of nitrate nitrogen is 2.0 mg/L or less, the amount of hardness is 50 mg/L ~ 200 mg/L, the amount of fluoride is 0.3 mg/L ~ 2.0 mg/L, there is no hazardous heavy metal and organic matter. A total of 64 items were investigated at 63 candidate sites: 46 items of the Korea drinking water standard; major elements (Ca, Mg, Na, K, Si), trace inorganic substance(Ge, Li, V, Se, Mo, Co, Ni, Ga, Be), and radioactive material (U, Rn). In order to select superior groundwater, the analysis results of each item at 63 sites were applied to the J-Index developed in 2017. As a result of this application, 10 sites were selected(Naju 2,  Goheung 2, Hwasun 2, Haenam 1, Yeongam 1, Yeonggwang 1, Jangseong 1). It is expected that the results of this study will contribute to the protection of precious water resources in Jeollanam-do.

본 연구에서는 수질이 우수하고 변동성이 적어 보존가치가 있는 우수 지하수를 전라남도 지정 명품지하수로 선정하기 위해 도내 개발·이용 중인 지하수를 대상으로 63개 후보지를 선정하였으며, 먹는물 46개 항목과 미네랄 성분, 기능성 미량성분 등을 분석하여 2017년도에 개발한 J-Index를 적용하여 평가한 결과는 다음과 같다.

1.  후보지 63개 지점의 항목별 농도 범위는 pH 5.9 ~ 8.5, 전기전도도 35 μS/cm ~ 878 μS/cm, 질산성질소(NO3-N) 불검출 ~ 5.6 mg/L, 불소(F-) 불검출 ~ 2.05 mg/L, 황산이온(SO42-) 1 mg/L~ 189 mg/L, 염소이온(Cl-) 1.0 mg/L ~ 47.5 mg/L, 경도 22 ~ 458 mg/L, 칼륨(K) 0.28 mg/L ~ 7.47 mg/L, 규소(Si) 0.49 mg/L ~ 20.90 mg/L, 마그네슘(Mg) 0.12 mg/L ~ 11.16 mg/L, 칼슘(Ca) 2.10 mg/L ~ 84.77 mg/L, 나트륨(Na) 3.46 mg/L ~ 61.44 mg/L, 미네랄 총량은 9.57 mg/L ~ 132.97 mg/L 게르마늄(Ge) 0.000 μg/L ~ 1.334 μg/L, 리튬(Li) 0.000 μg/L ~ 243.410 μg/L, 바나듐(V) 0.000 μg/L ~ 2.818 μg/L, 몰리브덴(Mo) 0.000 μg/L ~ 23.470 μg/L, 셀레늄(Se) 0.000 μg/L ~ 4.632 μg/L, 니켈(Ni) 0.000 μg/L ~ 1.842 μg/L, 우라늄(U) 불검출 ~ 5.397 μg/L로 조사되었으며, K-Index, O-Index 평가 결과, 건강에 좋고 맛있는 물(Group Ⅰ) 27개 지점, 건강에 좋은 물(Group Ⅱ) 12개 지점, 맛있는 물((Group Ⅲ) 19개 지점, 어느 쪽에도 속하지 않는 물(Group Ⅳ) 5개 지점으로 나타났다.

2.  명품지하수로 선정된 10개 지점의 항목별 농도 범위는 pH 7.3 ~ 8.5, 불소(F-) 0.27 mg/L ~ 1.13 mg/L, 질산성질소(NO3-N) 불검출 ~ 1.7 mg/L, 미네랄 총량은 48.91 mg/L ~ 132.97 mg/L, 몰리브덴(Mo) 1.103 μg/L ~ 20.295 μg/L, 리튬(Li) 14.292 μg/L ~ 103.679 μg/L, 바나듐(V) 0.000 μg/L ~ 1.560 μg/L, 게르마늄(Ge) 0.000 μg/L ~ 0.194 μg/L, 셀레늄(Se) 0.000 μg/L ~ 1.560 μg/L, 비소(As) 불검출, 우라늄(U) 불검출 ~ 1.306 μg/L로 조사되었으며, K-Index, O-Index 평가 결과, 건강에 좋고 맛있는 물(Group Ⅰ) 3개 지점, 건강에 좋은 물(Group Ⅱ) 5개 지점, 맛있는 물(Group Ⅲ) 2개 지점으로 나타났다.

3.  J-Index로 평가하여 선정한 명품지하수 10개소의 점수분포는 91.5점 ~ 87.5점으로 나타났다. 선정된 10개 지점은 고흥군 대서면, 고흥군 남양면에 위치한 소규모 급수시설 지하수, 장성군 황룡면에 위치한 마을상수도, 화순군 이서면에 위치한 소규모 급수시설 지하수, 영광군 불갑면에 위치한 공공지하수, 나주시 대호동에 있는 낙타봉 음수대, 나주시 경현동의 생태물놀이장에 위치한 음수대, 해남군 현산면에 위치한 마을상수도, 영암군 금정면에 위치한 마을상수도, 화순군 백아면에 위치한 마을상수도였다.

건강에 대한 관심이 고조되고 있는 사회적 분위기 속에 마시는 물에 대한 인식도 변화하면서 기능성 등을 내세워 다양한 종류의 마시는 물이 시판되고 있다. 본 연구는 전남지역 내 수질이 우수한 지하수를 발굴하여 그 가치를 재평가함으로써 전남의 소중한 수자원 보호에 기여할 뿐만 아니라 도민의 건강증진 및 지역발전에 도움이 될 것으로 기대된다. 아울러 2016년부터 연차적으로 시행하여 5년간 발굴한 전남지역 내 명품 지하수에 대해서 지속적인 모니터링을 통한 꾸준한 관리가 필요할 것으로 판단된다.